POSITION MEMORY CONTROL SYSTEM OPERATION

id091300959200

Position Memory Operation

1. A seat position memory signal is input to the position memory control module when memory operations are performed using the transmitter or seat memory switch.

2. When the seat memory control module receives a signal, the operation conditions are confirmed, and if the conditions are met, pulse signals from each motor are input to the memory circuit as seat positions and power outer mirror glass position.

3. When a seat position and power outer mirror glass position is input to the memory circuit, the buzzer sounds and the position memory operation is finished.

ac9wzn00000531

Position Memory Auto Call Up Operation

1. A seat position and power outer mirror glass position call up signal is input to the seat memory control module when an auto call up operation is performed using the transmitter or the seat memory switch.

2. When the position memory control module receives the signal, the operation conditions are confirmed, and if the conditions are met, the applicable seat position and power outer mirror glass are called up from the memory circuit to operate each motor and move the seat and power outer mirror glass to the applicable position.

ac9wzn00000532