MASS AIR FLOW (MAF)/INTAKE AIR TEMPERATURE (IAT) SENSOR REMOVAL/INSTALLATION [MZI-3.7]

id0140c3805500

  Note
  • The MAF sensor and IAT sensor cannot be removed as a single unit. When replacing the MAF sensor or IAT sensor, replace it together with the MAF/IAT sensor as a single unit.

1. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [MZI-3.7].)

2. Disconnect the MAF/IAT sensor connector.

3. Remove the MAF/IAT sensor.

ac9wzw00002358

4. Install in the reverse order of removal.