REAR END PANEL INSTALLATION [PANEL REPLACEMENT]

id098008744600

1. When installing new parts, measure and adjust the body as necessary to conform with standard dimensions.

2. Drill holes for the plug welding before installing the new parts.

3. Apply spot weld sealer to the joints of old and new parts for waterproofing and rust protection.

4. After temporarily installing new parts, make sure the related parts fit properly.

ac9uub00000067