REAR DOOR GLASS REMOVAL/INSTALLATION

id091200000300

1. To access the glass installation bolt, position the rear door glass so that the distance from the top of the rear door glass to the upper part of the rear beltline molding is approx. 140 mm {5.5 in}.

ac9uuw00000410

2. Disconnect the negative battery cable.

3. Remove the following parts:

  (1) Inner sail garnish (See INNER SAIL GARNISH REMOVAL/INSTALLATION.)

  (2) Rear door garnish (See REAR DOOR GARNISH REMOVAL/INSTALLATION.)

  (3) Rear door trim (See REAR DOOR TRIM REMOVAL/INSTALLATION.)

  (4) Rear door speaker (See REAR DOOR SPEAKER REMOVAL/INSTALLATION.)

4. Remove the bolts.

ac9wzw00001615

5. Remove the rear door glass guide and glass run channel as a single unit.

ac9wzw00001616

6. Remove the hole cover.

ac9wzw00001617

7. Remove the bolt.

8. Lift the rear door glass up and remove it in the direction of the arrow.

9. Install in the reverse order of removal.

  Note
  • When installing the rear door glass, align the glass edge with the glass run channel by hand through the speaker installation hole.