DOOR SASH FILM REMOVAL

id091600805200

1. Partially peel back the glass run channel.

2. Partially peel back the door weatherstrip.

3. Remove the following parts:

  (1) Inner garnish (See INNER GARNISH REMOVAL/INSTALLATION.)

  (2) Front door trim (See FRONT DOOR TRIM REMOVAL/INSTALLATION.)

  (3) Inner sail garnish (See INNER SAIL GARNISH REMOVAL/INSTALLATION.)

  (4) Rear door trim (See REAR DOOR TRIM REMOVAL/INSTALLATION.)

  (5) Front beltline molding (See FRONT BELTLINE MOLDING REMOVAL/INSTALLATION.)

  (6) Rear beltline molding (See REAR BELTLINE MOLDING REMOVAL/INSTALLATION.)

  (7) Front sash molding (See FRONT SASH MOLDING REMOVAL.)

  (8) Rear sash molding (See REAR SASH MOLDING REMOVAL.)

  (9) Rear door garnish (See REAR DOOR GARNISH REMOVAL/INSTALLATION.)

4. Peel off the rear sash film by pulling it outward from one end.

acxuuw00000914

  Note
  • Slowly remove the door sash film since it may tear easily.