ADVANCED KEYLESS ENTRY SYSTEM OPERATION

id091400595600

Normal Keyless Entry Function

Lock/unlock

  Note
  • If any of the following conditions are met, the doors cannot be locked by operating the advanced key.
    ― The auxiliary key is inserted in the ignition key cylinder.
    ― The start knob is not in the OFF position.
    ― The start knob is being pressed.
    ― Any door is open.
  • If any of the following conditions are met, the doors cannot be unlocked by operating the advanced key.
    ― The auxiliary key is inserted in the ignition key cylinder.
    ― The start knob is not in the OFF position.
    ― The start knob is being pressed.

1. When the advanced key is operated, the advanced key sends ID data and rolling code. They are received by the keyless receiver and sent to the keyless control module.

2. When the keyless control module receives a lock/unlock signal from the advanced key and verifies the ID, the signal is sent to the all lock actuators activate to lock/unlock.

3. The keyless control module operates the hazard warning lights flash to flash according to lock/unlock signal from the advanced key.

  ― When the LOCK button is pressed, the hazard warning lights flash once.
  ― When the UNLOCK button is operated, the hazard warning lights flash twice.

ac9wzn00000980

Advanced Keyless Entry Function

Door lock/unlock

  Note
  • If any of the following conditions are not met, the doors cannot be locked by operating the request switch.
    ― The advanced key is not inside the vehicle.
    ― All doors and trunk lid are closed.
    ― The auxiliary key is not inserted in the ignition key cylinder.
    ― The start knob is in the OFF position and not being pressed.
    ― The advanced key is within the reception range outside the vehicle.
  • If any of the following conditions are not met, the doors cannot be unlocked by operating the request switch.
    ― The auxiliary key is not inserted in the ignition key cylinder.
    ― The start knob is in the OFF position and not being pressed.
    ― The advanced key is within the reception range outside the vehicle.

1. When a request switch is pressed, the keyless control module sends a request signal from the keyless antenna. The request signal is sent to the area around the door that the request switch is pressed, and the signal is sent to the cabin area.

2. When the advanced key receives a request signal, the advanced key sends back ID data.

3. The ID data is received at the keyless receiver, and sent to the keyless control module.

4. When the ID data is verified by the keyless control module and the advanced key is determined to be outside the vehicle, a signal is sent to the BCM and all the lock actuators are activated to lock/unlock.

5. The keyless control module operates the hazard warning light to flash via the BCM.Allso, the keyless control module operates the keyless beeper at the same time.

  ― When the doors are locked, the hazard warning lights flash once.
  ― When the doors are unlocked, the hazard warning lights flash twice.

ac9wzn00000465

Auto re-lock function

  • The auto re-lock function automatically locks the doors if any of the following operations are performed within approx. 30 s after the UNLOCK button of the advanced key is pressed, or after the request switch is pressed to unlock the doors.
    ― A door or the liftgate is opened.
    ― The auxiliary key is inserted in the ignition key cylinder.
    ― The start knob is pressed.
    ― The advanced key is operated. (If the UNLOCK button is pressed, the timer is reset.)
    ― A request switch is operated.

Out-of-area (reception area) autolock function

  • When all doors are closed and the driver is out of the reception area carrying the advanced key, the doors are automatically locked. (Initial setting is OFF.)

1. When all the following conditions are met and all doors are closed after any door or the trunk lid is open, the keyless beeper sound is heard and the function starts operation. (The doors are not locked at this time.)

  ― The advanced key is not inside the vehicle.
  ― The advanced key is within the reception area outside the vehicle.
  ― The auxiliary key is not inserted in the ignition key cylinder.
  ― The start knob is in the OFF position, and not being pressed.

2. After the operation has started, the advanced key is monitored within the reception area by the keyless antenna. After about 2 s from where the advanced key has been determined to be out of the reception area, all lock actuators activate to lock. If approx. 30 s have passed since the operation started, the doors also locks regardless of whether the advanced key is within or out of the reception area.

3. The hazard warning light flashes once and keyless beep sound will be heard once at the same time the door locks.