DTC P0563:00 [MZI-3.7]

id0102d2156300

DTC P0563:00 | System voltage high
--- | ---
DETECTION CONDITION | • This DTC is stored when the PCM detects high system voltage.
POSSIBLE CAUSE | • Charging system concern.

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | VERIFY RELATED SERVICE INFORMATION AVAILABILITY • Verify related Service Information availability. • Is any related Service Information available? | Yes | Perform repair or diagnosis according to the available Service Information. • If the vehicle is not repaired, go to the next step.
No | Go to the next step.
2 | INSPECT THE CHARGING SYSTEM • Inspect the charging system. (See QUICK DIAGNOSTIC CHART [MZI-3.7].) • Is there any malfunction? | Yes | Repair or replace the malfunctioning part according to the inspection results, then go to the next step.
No | Go to the next step.
3 | VERIFY TROUBLESHOOTING OF DTC P0563:00 HAS BEEN COMPLETED • Verify that all disconnected connectors reconnected. • Clear the DTC from the PCM memory using the M-MDS. (See AFTER REPAIR PROCEDURE [MZI-3.7].) • Start the engine and run it at idle. • Retrieve DTCs using the M-MDS. • Is the same DTC present? | Yes | Repeat the inspection from Step 1. • If the malfunction recurs, replace the PCM. (See PCM REMOVAL/INSTALLATION [MZI-3.7].) Go to the next step.
No | Go to the next step.
4 | VERIFY AFTER REPAIR PROCEDURE • Perform the “AFTER REPAIR PROCEDURE”. (See AFTER REPAIR PROCEDURE [MZI-3.7].) • Are any DTCs present? | Yes | Go to the applicable DTC inspection. (See DTC TABLE [MZI-3.7].)
No | Troubleshooting completed.