PID/DATA MONITOR TABLE [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 8-PIN TYPE]

id0902q2960700

—: Not applicable

PID name | Unit/Operation | Data contents | Inspection item(s)
--- | --- | --- | ---
BSM_ST (BSM OFF switch) | Off/On | • When the BSM at off: Off • When the BSM at on: On | BSM OFF switch
BSM_OFF_IL*2 (BSM OFF indicator light) | Off/On | • When the BSM OFF indicator light is turned off: Off • When the BSM OFF indicator light is illuminated: On | Instrument cluster
Buzzer (Buzzer) | Off/On | • When the buzzer is not operating: Off • When the buzzer is operating: On | Instrument cluster
DTC_CNT (Number of continuous DTCs) | — | Indicates the number of DTC. | —
SHIFT_R (Selector lever position (Reverse)) | Not_R/R | • When the selector lever position is not R: Not_R • When the selector lever position is R: R | Back-up light relay
SWA_POS (Steering wheel angle) | ° (deg) | • Steering wheel in neutral position (not turned): 0 • Steering wheel turned to left: Changes 0—negative • Steering wheel turned to right: Changes 0—positive | Steering angle sensor
TURN_SW_L (Turn switch (LH)) | Off/On | • Turn switch is in the off position: Off • Turn switch is in the LH position: On | Turn switch
TURN_SW_R (Turn switch (RH)) | Off/On | • Turn switch is in the off position: Off • Turn switch is in the RH position: On | Turn switch
VPWR_IG1 (Module supply voltage) | V | Indicates the BSM control module power supply voltage. | BSM control module
VSPD (Vehicle speed) | KPH {MPH} | Indicates the vehicle speed. | —
WRN_IND_L*1 (BSM indicator light (LH)) | Off/On | • When the BSM indicator light (LH) is off: Off • When the BSM indicator light (LH) is illuminated: On | BSM indicator light (LH)
WRN_IND_R*2 (BSM indicator light (RH)) | Off/On | • When the BSM indicator light (RH) is off: Off • When the BSM indicator light (RH) is illuminated: On | BSM indicator light (RH)

*1 :BSM control module (LH)
*2 :BSM control module (RH)