AUTO LEVEL CONTROL (ALC) OPERATION

id092000106800

• The audio unit changes the volume automatically based on the vehicle speed signal sent from the instrument cluster.

acxuun00000364

• The ALC function is divided into 7 levels. When the level is in the high range, the volume correction range and correction amount is large. The maximum correction amount is 14dB. The ALC function can be stopped by selecting ALC OFF.

am5ezn00002051