DTC TABLE [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 8-PIN TYPE]

id0902q2347100

DTC No. | Detection condition | Description | Page
--- | --- | --- | ---
B118C:11*1 | • The BSM control module (LH) monitors the BSM indicator light (LH) load current, while the BSM indicator light (LH) is operating. When the increase in the BSM indicator light (LH) load current is more than the specification, the BSM control module (LH) determines that the BSM indicator light (LH) has a short to ground. | Short to ground in BSM indicator light (LH) circuit | (See DTC B118C:11 [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 8-PIN TYPE].)
B118C:15*1 | • The BSM control module (LH) monitors the BSM indicator light (LH) load current, while the BSM indicator light (LH) is operating. If the decrease in the BSM indicator light (LH) load current is less than the specification, the BSM control module (LH) determines that the BSM indicator light (LH) has an open circuit or short to power supply. | Short to power supply or open circuit in BSM indicator light (LH) circuit | (See DTC B118C:15 [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 8-PIN TYPE].)
B118D:11*2 | • The BSM control module (RH) monitors the BSM indicator light (RH) load current, while the BSM indicator light (RH) is operating. If the increase in the BSM indicator light (RH) load current is more than the specification, the BSM control module (RH) determines that the BSM indicator light (RH) has a short to ground. | Short to ground in BSM indicator light (RH) circuit | (See DTC B118D:11 [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 8-PIN TYPE].)
B118D:15*2 | • The BSM control module (RH) monitors the BSM indicator light (RH) load current, while the BSM indicator light (RH) is operating. If the decrease in the BSM indicator light (RH) load current is less than the specification, the BSM control module (RH) determines that the BSM indicator light (RH) has an open circuit or short to power supply. | Short to power supply or open circuit in BSM indicator light (RH) circuit | (See DTC B118D:15 [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 8-PIN TYPE].)
U0001:88 | • BSM control module detects a CAN bus communication line (HS-CAN) malfunction for 0.4 s or more. | Module communication error (HS-CAN) | (See FOREWORD [MULTIPLEX COMMUNICATION SYSTEM (L.H.D.)].) (See FOREWORD [MULTIPLEX COMMUNICATION SYSTEM (R.H.D.)].)
U0100:00 | • BSM control module cannot receive the CAN signal from the PCM for 1 s or more. | Communication error with PCM
U0101:00 | • BSM control module cannot receive the CAN signal from the TCM for 1 s or more. | Communication error with TCM
U0140:00 | • BSM control module cannot receive the CAN signal from the BCM for 1 s or more. | Communication error with BCM
U0232:00*2 | • BSM control module (RH) cannot receive the CAN signal from the BSM control module (LH) for 1 s or more. | Communication error with BSM control module (LH)
U0233:00*1 | • BSM control module (LH) cannot receive the CAN signal from the BSM control module (RH) for 1 s or more. | Communication error with BSM control module (RH)
U0401:68 | • BSM control module receives the error signal from the PCM for 1 s or more. | Error signal from PCM | (See DTC U0401:68 [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 8-PIN TYPE].)
U0402:68 | • BSM control module receives the error signal from the TCM for 1 s or more. | Error signal from TCM | (See DTC U0402:68 [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 8-PIN TYPE].)
U0422:68 | • BSM control module receives the error signal from the BCM for 1 s or more. | Error signal from BCM | (See DTC U0422:68 [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 8-PIN TYPE].)
U0533:68*2 | • BSM control module (RH) receives the error signal from the BSM control module (LH) for 1 s or more. | Error signal from BSM control module (LH) | (See DTC U0533:68 [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 8-PIN TYPE].)
U0534:68*1 | • BSM control module (LH) receives the error signal from the BSM control module (RH) for 1 s or more. | Error signal from BSM control module (RH) | (See DTC U0534:68 [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 8-PIN TYPE].)
U3000:01 | • BSM control module detects the internal electrical malfunction. | BSM control module internal electrical malfunction | (See DTC U3000:01 [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 8-PIN TYPE].)
U3000:09 | • BSM control module detects the malfunction of voltage control oscillator in the BSM control module. | BSM control module internal malfunction | (See DTC U3000:09 [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 8-PIN TYPE].)
U3000:4A | • A logic is provided to monitor for incorrect installation in order to prevent the left and right BSM control modules from being installed in reverse of each other. Terminal E of the BSM control module (LH) monitors the body ground condition, and terminal E of the BSM control module (RH) monitors the BSM OFF switch condition. The circuit is open during non-operation of the BSM OFF switch. It can be determined that the left and right BSM control modules have been installed in reverse if the following conditions occur: ― A short to ground condition of BSM control module (RH) terminal E continues for 180 s or more. ― An open circuit condition of BSM control module (LH) terminal E continues for 0.9 s or more. | BSM control module assembly abnormality | (See DTC U3000:4A [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 8-PIN TYPE].)
U3000:97 | • BSM control module detects the radar sensor sensitivity decrease. • BSM control module detects the radar sensor axial deviation. | BSM control module radar performance malfunction | (See DTC U3000:97 [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 8-PIN TYPE].)
U3003:16 | • BSM control module power supply voltage is less than 9 V for 10 s or more. | BSM control module power supply voltage low input | (See DTC U3003:16/U3003:17 [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 8-PIN TYPE].)
U3003:17 | • BSM control module power supply voltage is 16 V or more for 10 s or more. | BSM control module power supply voltage high input

*1 :BSM control module (LH)
*2 :BSM control module (RH)