COMPONENT DESCRIPTIONS (ELECTRONIC CONTROL) [AY6A-EL, AY6AX-EL]

id0517k3223600

Part name | Function
--- | ---
Input system | M position switch | • Selects driving modes (M position) and changes driving patterns.
Up switch | • Detects shift up request.
Down switch | • Detects shift down request.
TR switch | • Detects selector lever positions.
APP sensor | • Detects the accelerator pedal depressing amount.
Input/turbine speed sensor | • Detects the C2 clutch drum (input) revolution speed.
VSS | • Detects the counter drive gear (output) revolution speed.
Brake switch | • Detects the use of service brake.
TFT sensor | • Detects the ATF temperature.
CHT sensor | • Detects the engine cylinder head temperature. The PCM calculates the engine coolant temperature based on the signal.
CKP sensor | • Detects the engine revolution speed.
MAF sensor | • Detects the intake air amount.
ABS wheel-speed sensor | • Detects the wheel speed.
Output system | Linear type | Line pressure control solenoid | • Adjusts the line pressure.
Shift solenoid C | • Controls the clutch engagement pressure.
Shift solenoid D | • Controls the clutch engagement pressure.
Shift solenoid E | • Controls the clutch engagement pressure.
Shift solenoid F | • Controls the clutch engagement pressure.
TCC control solenoid | • Controls the TCC and slip hydraulic pressure.
3-way type | Shift solenoid A | • Controls the clutch engagement pressure.
Shift solenoid B | • Controls the clutch engagement pressure.
AT warning light | • Illuminates when failure is detected by diagnosis function.
Speedometer signal | • Outputs the vehicle speed signal to speedometer.