MASTER CYLINDER REMOVAL/INSTALLATION [R.H.D.]

id041100801352

1. Remove the engine cover. (See BATTERY REMOVAL/INSTALLATION [MZI-3.7].)

2. Remove in the order indicated in the table.

3. Install in the reverse order of removal.

4. After installation, add brake fluid, bleed the air, and inspect for fluid leakage. (See AIR BLEEDING.)

ac9wzw00003280

1 | Brake fluid level sensor connector
2 | Brake pipe
3 | Master cylinder component
4 | Master cylinder bracket
5 | Brake fluid level sensor short cord
6 | O-ring