NO.3 VEHICLE POSITION DEVIATES FROM THE ROUTE MAP [CAR-NAVIGATION SYSTEM]

id0903e8833600

3 | The vehicle position on the map screen deviates from the actual vehicle position.
--- | ---
Possible DTC | —
POSSIBLE CAUSE | • GPS antenna malfunction • Car-navigation unit malfunction • Audio unit malfunction • Poor GPS antenna connection • Poor reception due to object obstructing GPS antenna

Diagnostic Procedure

Step | Inspection | Action
--- | --- | ---
1 | VERIFY GPS ANTENNA RECEPTION CONDITION • Stop the vehicle and leave it idling for 5 min in an area with clear visibility (no buildings or trees surrounding). • Verify the GPS signal reception condition on the audio unit screen. (See Procedure for Displaying GPS status screen.) • Is the GPS information displayed on the GPS status screen?
am6zzw00012225
Note • If 4 or more satellites are displayed, the GPS signal reception strength is normal. | Yes | Replace the car-navigation unit. (See CAR-NAVIGATION UNIT REMOVAL/INSTALLATION.)
No | Go to the next step.
2 | VERIFY IF GPS ANTENNA RECEPTION IS OBSTRUCTED • Is there an object on the dashboard which is interfering with GPS reception (such as devices installed by customer after installation)? | Yes | After explaining to the customer that device installed by the customer on the dashboard after the installation is interfering with GPS reception, remove the device. After servicing, go to the next step.
No | Go to the next step.
3 | VERIFY THE GPS ANTENNA RECEPTION SIGNAL • Launch the audio unit diagnostic assist function. (See DIAGNOSTIC ASSIST FUNCTION [AUDIO].) • Select diagnostic assist code 15 vehicle NAVI signal verification. • Is NAVI GPS ANT NG displayed? | Yes | Go to the next step.
No | Replace the car-navigation unit. (See CAR-NAVIGATION UNIT REMOVAL/INSTALLATION.)
4 | VERIFY GPS ANTENNA CONNECTOR CONDITION • Switch the ignition off. • Disconnect the negative battery cable. • Disconnect the GPS antenna connector. • Inspect the connector and terminals (connection condition, corrosion, damage, pin disconnection). • Are the connectors and terminals normal? | Yes | Go to the next step.
No | Repair or replace the pins, connectors.
5 | VERIFY CAR-NAVIGATION UNIT CONNECTOR CONDITION • Disconnect the car-navigation unit connector. • Inspect the connector and terminals (connection condition, corrosion, damage, pin disconnection). • Are the connectors and terminals normal? | Yes | Go to the next step.
No | Repair or replace the pins, connectors.
6 | INSPECT FOR SHORT TO GROUND IN WIRING HARNESS BETWEEN GPS ANTENNA AND CAR-NAVIGATION UNIT • Inspect for continuity between the following terminals (vehicle wiring harness side) and body ground. ― GPS antenna terminal A • Is there continuity? | Yes | Repair or replace the wiring harness, then go to Step 10.
No | Go to the next step.
7 | INSPECT FOR OPEN CIRCUIT IN WIRING HARNESS BETWEEN GPS ANTENNA AND CAR-NAVIGATION UNIT • Inspect the wiring harness between the following terminals (vehicle wiring harness side) for continuity. ― GPS antenna terminal A and car-navigation unit terminal B (2-pin) • Is there continuity? | Yes | Go to the next step.
No | Repair or replace the wiring harness, then go to Step 10.
8 | INSPECT FOR SHORT TO POWER SUPPLY IN WIRING HARNESS BETWEEN GPS ANTENNA AND CAR-NAVIGATION UNIT • Connect the negative battery cable. • Switch the ignition ON (engine off or on). • Measure the voltage at the following terminals (vehicle wiring harness side). ― GPS antenna terminal A • Is the voltage 0 V? | Yes | Replace the GPS antenna. (See GLOBAL POSITIONING SYSTEM (GPS) ANTENNA REMOVAL/INSTALLATION.)
No | Replace the car-navigation unit. (See CAR-NAVIGATION UNIT REMOVAL/INSTALLATION.)

Procedure for Displaying GPS status screen

1. Display the Main menu screen shown in the figure.

am6zzw00012222

2. Select “Settings” on the Main menu screen.

3. Select “Status & Information” on the Settings screen.

am6zzw00012223

4. Select “GPS status” on the Status & Information screen.

am6zzw00012224