FRONT FENDER PANEL REMOVAL/INSTALLATION

id091000801000

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Windshield wiper arm and blade (See WINDSHIELD WIPER ARM AND BLADE REMOVAL/INSTALLATION)

  (2) Side cowl grille (See COWL GRILLE REMOVAL/INSTALLATION)

  (3) Front over fender (See OVER FENDER REMOVAL/INSTALLATION)

  (4) Front bumper (See FRONT BUMPER REMOVAL/INSTALLATION)

  (5) Front combination lights (See FRONT COMBINATION LIGHT REMOVAL/INSTALLATION)

  (6) Sail garnish (See SAIL GARNISH REMOVAL/INSTALLATION)

3. Remove in the order indicated in the table.

ac9uuw00000874

1 | Screw
2 | Front bumper retainer
3 | Bolt A
4 | Bolt B
5 | Bolt C
6 | Bolt D
7 | Bolt E
8 | Clip
9 | Seal plate
10 | Front fender panel

4. Install in the reverse order of removal.