THIRD-ROW BUCKLE REMOVAL/INSTALLATION

id081100802300

Removal

1. Fold the third-row seat backs forward.

2. Remove the trunk box. (See TRUNK BOX REMOVAL/INSTALLATION.)

3. Remove the bolt.

ac9uuw00000325

4. Remove the third-row buckle.

Installation

1. Bind the third-row seat belt buckles in a band as shown in the figure.

ac9uuw00002476

2. Install the bolt.

ac9wzw00000950

3. Remove the trunk box. (See TRUNK BOX REMOVAL/INSTALLATION.)