FRONT OUTER HANDLE REMOVAL/INSTALLATION

id091400803100

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Inner garnish (See INNER GARNISH REMOVAL/INSTALLATION.)

  (2) Front door trim (See FRONT DOOR TRIM REMOVAL/INSTALLATION.)

  (3) Front door speaker (See FRONT DOOR SPEAKER REMOVAL/INSTALLATION.)

  (4) Front door glass (See FRONT DOOR GLASS REMOVAL/INSTALLATION.)

  (5) Front door module (See FRONT DOOR MODULE PANEL REMOVAL/INSTALLATION.)

3. Disconnect the rod from the front outer handle.

4. Disconnect the rod from the front door key cylinder. (Driver side)

ac9uuw00002323

5. Remove the bolt.

ac9uuw00001242

6. Remove the front door key cylinder. (Driver side) (See FRONT DOOR KEY CYLINDER REMOVAL/INSTALLATION.)

7. Secure the rear part of the front outer handle and, with the front outer handle lever pulled outward (1), remove the rear part of the front outer handle from the front door.

acxuuw00002479

8. Pull out the front side of the front outer handle from the front door.

9. Install in the reverse order of removal.