POWER WINDOW SUBSWITCH REMOVAL/INSTALLATION

id091200002200

Passenger-side

1. Disconnect the negative battery cable.

2. Remove the inner garnish. (See INNER GARNISH REMOVAL/INSTALLATION.)

3. Remove the front door trim. (See FRONT DOOR TRIM REMOVAL/INSTALLATION.)

4. Remove the screw, and remove the power window subswitch from inside the front door trim.

ac9wzw00001643

5. Install in the reverse order of removal.

Rear-side

1. Disconnect the negative battery cable.

2. Remove the inner sail garnish. (See INNER SAIL GARNISH REMOVAL/INSTALLATION.)

3. Remove the rear door trim. (See REAR DOOR TRIM REMOVAL/INSTALLATION.)

4. Remove the screw, and remove the power window subswitch from inside the rear door trim.

ac9wzw00001644

5. Install in the reverse order of removal.