DSC/RSC SENSOR INITIALIZATION PROCEDURE

id041800816400

  Warning
  • Unless the initialization procedure of the DSC/RSC HU/CM is completed, the DSC/RSC will not operate, causing an unexpected accident. Therefore, always perform the initialization procedure to ensure DSC/RSC operation if the DSC/RSC HU/CM or SAS control module have been removed or replaced.

1. Inspect the wheel alignment and inflation pressure.

  • If there is any malfunction, adjust the applicable part.

2. Park the vehicle on level ground.

3. Turn the ignition switch to the OFF position.

4. Connect the M-MDS to the DLC-2.

ac9uuw00000862

5. After the vehicle is identified, select the following items from the initialization screen of the M-MDS.

  • When using the IDS (laptop PC)
    1. Select “Chassis”.
    2. Select “ABS/DSC”.
    3. Select “Sensor Initialization”.

  • When using the PDS (Pocket PC)
    1. Select “Module Test”.
    2. Select “ABS”.
    3. Select “Datalogger”.
    4. Select “SSR_INTL”.

6. Perform the initialization according to the directions on the screen.