REAR AUTO LEVELING SENSOR REMOVAL/INSTALLATION

id091800806900

1. Disconnect the negative battery cable.

2. Jack up the vehicle.

3. Remove the wheels and tire (LH). (See GENERAL PROCEDURES (SUSPENSION).)

4. Disconnect the connector.

5. Remove the nut.

ac9wzw00001266

6. Install in the reverse order of removal.

7. Perform the auto leveling system initialization. (See AUTO LEVELING SYSTEM INITIALIZATION.)