CUSTOMIZED FUNCTION SETTING PROCEDURE [ADVANCED KEYLESS ENTRY AND START SYSTEM]

id0914008074z6

Using M-MDS

1. Connect the M-MDS to the DLC-2.

ac9uuw00000452

2. After the vehicle is identified, select the following items from the initial screen of the M-MDS.

  1. Select the “Module Programming”.

3. Then, select items from the screen menu in the following order.

  1. Select “Programmable Parameters”.
  2. Select “RKE(Remote Keyless Entry)”.

4. Select an item name, and then select option.

  Caution
  • Do not change customized function which are not indicated in the workshop manual.

Mazda Modular Diagnostic System (M-MDS) display | Function | Initial setting | Setting content | Control unit
--- | --- | --- | --- | ---
Answer Back Buzzer | Answer back buzzer function can be set. | Enabled | Disabled/ Enabled | Keyless control module
Card key battery low warning | Advanced key remaining battery level/battery dead warning can be set. | Enabled | Disabled/ Enabled | Keyless control module
Automatic Locks | Automatic locks function can be set. | Disabled | Disabled/ Enabled | Keyless control module
Two(2) stage door unlocking by request switch. | 2-step unlocking system can be set. | Enabled | Disabled/ Enabled | Keyless control module
Two(2) stage door unlocking by transmitter. | 2-step unlocking system can be set. | Enabled | Disabled/ Enabled | Keyless control module
Auto relock timer (with AKE) | The operation start time of the auto re-lock function can be changed. | 60s | 30s/60s/90s | Keyless control module

Setting Method By Operation Of Door Lock Switch

Auto door lock system

Setting content | Function | Initial setting | Control unit
--- | --- | --- | ---
Disabled | Auto lock/unlock function can be changed. | Auto door lock operation based on vehicle speed. Auto door unlock operation based on ignition switch position. | BCM
Auto door lock operation based on vehicle speed.
Auto door lock operation based on vehicle speed. Auto door unlock operation based on ignition switch position.
Auto door lock operation based on shift position.
Auto door lock operation based on shift position. Auto door unlock operation based on shift position.

Setting procedure

ac9wzw00003166