BLIND SPOT MONITORING (BSM) CONTROL MODULE REMOVAL/INSTALLATION [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 8-PIN TYPE]

id0922008100e1

  Caution
  • If the BSM control modules are installed with the left and right modules reversed, a DTC will be displayed and system will enter the fail-safe function. Therefore, confirm that the left/right BSM control modules are installed correctly.

1. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [MZI-3.7].)

2. Remove the rear combination light. (See REAR COMBINATION LIGHT REMOVAL/INSTALLATION.)

3. Remove the rear bumper. (See REAR BUMPER REMOVAL/INSTALLATION.)

4. Pull the connector in the direction shown by the arrow (2) in the figure and remove it while pressing the tab in the direction shown by arrow (1).

ac9uuw00002662

5. Remove the nuts.

6. Remove the BSM control module.

7. Install in the reverse order of removal.

8. Perform the blind spot monitoring radar test. (See BLIND SPOT MONITORING (BSM) RADAR TEST [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 8-PIN TYPE].)