DTC B1506 [BCM]

id0902f5831600

Description | Turn switch (RH) circuit malfunction
--- | ---
Detection condition | • Short to ground in turn switch (RH) circuit with the turn switch off.
Possible cause | • Light switch connector or terminal malfunction • Turn switch malfunction • BCM connector or terminal malfunction • Short to ground in wiring harness between the following terminals: ― Light switch terminal E—BCM terminal 3G (L.H.D.) ― Light switch terminal Q—BCM terminal 3G (R.H.D.) • BCM malfunction

Diagnostic procedure

Step | Inspection | Action
--- | --- | ---
1 | INSPECT LIGHT SWITCH CONNECTOR • Turn the ignition switch to the OFF position. • Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [MZI-3.7].) • Disconnect the light switch connector. • Inspect the connector engagement and connection condition and inspect the terminals for damage, deformation, corrosion, or disconnection. • Is there any malfunction? | Yes | Repair or replace the connector, then go to Step 5.
No | Go to the next step.
2 | INSPECT TURN SWITCH • Inspect the turn switch. (See LIGHT SWITCH INSPECTION.) • Is there any malfunction? | Yes | Replace the light switch, then go to Step 5. (See LIGHT SWITCH REMOVAL/INSTALLATION.)
No | Go to the next step.
3 | INSPECT BCM CONNECTOR • Disconnect the BCM connector. • Inspect the connector engagement and connection condition and inspect the terminals for damage, deformation, corrosion, or disconnection. • Is there any malfunction? | Yes | Repair or replace the connector, then go to Step 5.
No | Go to the next step.
4 | INSPECT FOR SHORT TO GROUND IN TURN SWITCH (RH) CIRCUIT • Verify that the light switch and BCM connectors are disconnected. • Inspect for continuity between following terminal (wiring harness-side) and body ground: ― Light switch terminal E (L.H.D.) ― Light switch terminal Q (R.H.D.) • Is there continuity? | Yes | Repair or replace the wiring harness which has a short to ground, then go to the next step.
No | Go to the next step.
5 | VERIFY DTC TROUBLESHOOTING COMPLETED • Make sure to reconnect all disconnected connectors. • Reconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [MZI-3.7].) • Clear the DTC for the BCM using the M-MDS. (See CLEARING DTC [BCM].) • Retrieve the BCM DTCs using the M-MDS. (See DTC INSPECTION [BCM].) • Is the same DTC displayed? | Yes | Repeat the inspection from Step 1. • If the malfunction recurs, replace the BCM. (See BODY CONTROL MODULE (BCM) REMOVAL/INSTALLATION.) Go to the next step.
No | Go to the next step.
6 | VERIFY IF OTHER DTCs DISPLAYED • Are any other DTCs displayed? | Yes | Repair or replace the malfunctioning part according to the applicable DTC troubleshooting. (See DTC TABLE [BCM].)
No | DTC troubleshooting completed.