POWER LIFTGATE (PLG) BUZZER REMOVAL/INSTALLATION

id091100001900

  Caution
  • Do not remove the PLG buzzer except when replacing the PLG buzzer because thread-locking compound has been applied to the screws.

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Liftgate upper trim (See LIFTGATE UPPER TRIM REMOVAL/INSTALLATION.)

  (2) PLG arm (See POWER LIFTGATE (PLG) DRIVE UNIT REMOVAL/INSTALLATION.)

  (3) Liftgate side trim (See LIFTGATE SIDE TRIM REMOVAL/INSTALLATION.)

  (4) Liftgate lower trim (See LIFTGATE LOWER TRIM REMOVAL/INSTALLATION.)

3. Disconnect the PLG buzzer connector.

ac9wzw00001042

4. Remove the bolt.

5. Remove the clip.

6. Remove the PLG buzzer.

7. Install in the reverse order of removal.