COWL GRILLE REMOVAL/INSTALLATION

id091600801000

1. Remove the windshield wiper arm and blade. (See WINDSHIELD WIPER ARM AND BLADE REMOVAL/INSTALLATION.)

2. Remove the fastener then remove the front fender molding.

ac9uuw00000825

3. Remove the weatherstrip.

4. Remove the fastener.

5. Remove the side cowl grille.

6. Pull the cowl grille in the direction of arrow (1) so that it is free from the pins, pull tabs A in the direction of arrow (2), and then remove the windshield.

7. Disconnect the windshield washer hose.

ac9uuw00001176

8. Remove the cowl grille.

9. Install in the reverse order of removal.