REAR FINISHER REMOVAL/INSTALLATION

id091600800200

1. Remove the liftgate upper trim. (See LIFTGATE UPPER TRIM REMOVAL/INSTALLATION)

2. Remove the liftgate side trim. (See LIFTGATE SIDE TRIM REMOVAL/INSTALLATION)

3. Remove the liftgate lower trim. (See LIFTGATE LOWER TRIM REMOVAL/INSTALLATION.)

4. Set the noise filter out of the way. (See NOISE FILTER REMOVAL/INSTALLATION.)

5. Remove the bolts.

ac9uuw00002350

6. Remove the dynamic damper.

7. Disconnect the request switch connector and the rear mount camera connector.

ac9wzw00003018

8. Remove the nuts.

9. Pull the rear finisher outward, then disengage clip A, B, and C from the body.

10. Remove the rear finisher.

11. Remove the request switch. (Vehicles with advanced keyless system) (See REQUEST SWITCH REMOVAL/INSTALLATION [ADVANCED KEYLESS ENTRY AND START SYSTEM].)

12. Remove the rear mount camera. (Vehicles with rear mount camera) (See REAR MOUNT CAMERA REMOVAL/INSTALLATION.)

13. Install in the reverse order of removal.