HVAC SPECIFICATIONS

id070000100300

Basic system

Item | Specification
--- | ---
FRONT | REAR
Heating capacity | (kW {kcal/h}) | 5.250 {4,515} | 2.0 {1,720}
Cooling capacity | (kW {kcal/h}) | 4.360 {3,749} | 1.290 {1,109}
Refrigerant | Type | R-134a
Regular amount (approx. quantity) | (g {oz}) | 660—710 {23.3—25.0}
A/C compressor | Type | Swash plate
Discharge capacity | (ml {cc, fl oz}) | 214.7 {214.7, 7.26}
Max. allowable speed | (rpm) | 6,000
Lube oil | Type | DENSO OIL8
Sealed volume (approx. quantity) | (ml {cc, fl oz}) | 160 {160, 5.41}
Condenser | Type | Multiflow (sub-cooling type)
Radiated heat | (kW {kcal/h}) | 9.0 {7,740}
Receiver/drier capacity | (ml {cc, fl oz}) | 280 {280, 9.46}
Desiccant | XH-9
Expansion valve | Type | External equalizing type | External equalizing type
Evaporator | Type | Double-tank drawn cup | Double-tank drawn cup

Control system

Item | Specification
--- | ---
FRONT | REAR
Airflow volume (during heater operation) | Blower motor | (m3/h) | 330 | 120
Electricity consumption (during heater operation) | Blower motor | (W) | 220 | 130
Airflow volume (during air conditioner operation) | Blower motor | (m3/h) | 515 | 240
Electricity consumption (during air conditioner operation) | Blower motor | (W) | 250 | 130
Magnetic clutch | (W) | 35
Magnetic clutch clearance (approx. quantity) | (mm {in}) | 0.35—0.60 {0.014—0.024}
Fan type | Blower motor | Sirocco fan | Sirocco fan
Refrigerant pressure sensor | Type | Capacitance type
Sensor operation | (See REFRIGERANT PRESSURE SENSOR CONSTRUCTION [FULL-AUTO AIR CONDITIONER].)
Sensor | Solar radiation sensor | Photodiode
Ambient temperature sensor | Thermistor
Cabin temperature sensor | Thermistor | Thermistor
Evaporator temperature sensor | Thermistor | Thermistor
Actuator | Air intake actuator | Sliding contact type
Air mix actuator | Potentiometer type | Potentiometer type
Airflow mode actuator | Potentiometer type | Potentiometer type