BLIND SPOT MONITORING (BSM) OFF SWITCH INSPECTION

id092200810400

1. Disconnect the negative battery cable.

2. Remove the BSM OFF switch. (See BLIND SPOT MONITORING (BSM) OFF SWITCH REMOVAL/INSTALLATION.)

3. Verify that the continuity is as indicated in the table.

ac9wzw00002683

  • If not as indicated in the table, replace the cluster switch.

4. Apply battery positive voltage to BSM OFF switch terminal E, and connect terminal A to ground.

ac9wzw00002684

5. Verify that the LED illuminates.

  • If there is any malfunction, replace the cluster switch.