ADVANCED KEYLESS ENTRY AND START SYSTEM OUTLINE

id091400594200

• An advanced keyless system has been adopted that enables the driver to start the engine or lock/unlock the doors without operating the key or transmitter (advanced key) by carrying the card key that has been programmed to the vehicle.
• The doors also can be locked/unlocked by operating the key (auxiliary key) or transmitter (advanced key).
• The answer-back function has been adopted where the hazard warning light flashes and a beeping sound confirms that the doors are locked/unlocked. Also, the advanced keyless entry system indicates activation by a beeper sound.
• A warning and guidance function has been adopted that promotes correction if the system is operated improperly, and uses the indicator light in the instrument cluster, a beeper sound, and the keyless beeper from behind passenger compartment.
• A customize function that switches the activation/deactivation of each function has been adopted.
• A rolling code type transmitter (advanced key) has been adopted to prevent theft by radiowave interception.
• To prevent improper operation while the vehicle is moving, the doors cannot be locked/unlocked by operating the transmitter (advanced key) or request switch when the start knob is in any position except OFF.