FRONT POWER METAL OXIDE SEMICONDUCTOR FIELD EFFECT TRANSISTOR (POWER MOS FET) INSPECTION

id074000803700

1. Verify that the continuity between the front power MOS FET terminals is as indicated in the table.

  • If there is any malfunction, replace the front power MOS FET.
  • If the blower motor operation is not normal even though no malfunction can be verified, inspect the front climate control unit.

ac9wzw00001707

Tester lead | Resistance (kilohm)
--- | ---
+ | -
A | B | 2.2
A | E | Continuity detected
A | F | Continuity detected
B | A | 2.2
B | E | Continuity detected
B | F | Continuity detected
E | A | ∞
E | B | ∞
E | F | 11
F | A | ∞
F | B | ∞
F | E | 11