REAR MOUNT CAMERA CONSTRUCTION/OPERATION

id092000109800

• The rear mount camera is located in the liftgate.

ac9wzn00000911

• A super-wide angle lens which can shoot images in a wide parameter is assembled to the compact (1/3.6 in), color CMOS camera which has a high precision CMOS*1 imaging element.
*1 :Complementary Metal-Oxide Semiconductor

Displayable Range

  Note
  • Some of the guidelines for the back camera are displayed and not displayed on the screen depending on the vehicle's period of manufacture.

• The displayable range varies depending on the vehicle and road conditions.
• The displayable range is limited. Objects under the bumper or around the bumper ends cannot be displayed.
• The distance appearing in the displayed image is different from the actual distance because the rear mount camera is equipped with a specific lens.

ac9wzn00000445

No. | Display item | color | Function
--- | --- | --- | ---
1 | Distance reference lines (fixed) | Red | • Shows distance reference line 0.5 m from the rear of the rear bumper. • Not in conjunction with steering operation.
2 | Yellow | • Shows distance reference line 1.0 m from the rear of the rear bumper. • Not in conjunction with steering operation.
3 | Yellow | • Shows distance reference line 2.7 m from the rear of the rear bumper. • Not in conjunction with steering operation.
4 | Vehicle width extension line | Yellow | • Vehicle width extension line. (Length: 2.7 m, width: vehicle width)

• Same optionally installed vehicle accessories, such as illuminating parts or parts made of reflective material, may be picked up by the rear mount camera. Do not install any optional parts or accessories that could interfere with the rear mount camera display.
• It may be difficult to see the display under the following conditions; however, it does not indicate a malfunction:

  ― In darkened areas.
  ― When the temperature around the lens is high/low.
  ― When the camera is wet such as on a rainy day or during period of high humidity.
  ― When foreign material such as mud is stuck around the camera.
  ― When the camera lens reflects sunlight or headlight beams.

• If the camera picks up a high-intensity light such as sunlight reflected off the vehicle body, a bright belt (light line) may appear on the display (Smear phenomenon).
• Image display may be delayed if the temperature around the rear mount camera is low.