BONNET REMOVAL/INSTALLATION

id091000802500

  Warning
  • Removing the bonnet without supporting it could cause the bonnet to fall and cause serious injury. Always perform the procedure with at least another person to prevent the bonnet from falling.

1. Disconnect the negative battery cable.

2. To remove the bonnet hinges, remove the following parts:

  (1) Windshield wiper arm and blade (See WINDSHIELD WIPER ARM AND BLADE REMOVAL/INSTALLATION)

  (2) Side cowl grille (See COWL GRILLE REMOVAL/INSTALLATION)

3. Remove in the order indicated in the table.

ac9uuw00004631

1 | Bonnet insulator
2 | Shroud seal weatherstrip
3 | Parting seal weatherstrip
4 | Bonnet
5 | Bonnet hinge
6 | Bonnet stay

4. Install in the reverse order of removal.

5. Adjust the bonnet. (See BONNET ADJUSTMENT.)