ELECTRONIC CONTROL COUPLING OUTLINE

id031800166400

Features

• An electromagnetic clutch, which operates smoothly due to the lack influence from the front and rear wheel traction force, has been adopted for the electronic control coupling system.
• The construction of the coupling enables the torque formed by the pilot clutch to be amplified by the cam mechanism, thus allowing the main clutch to obtain a high degree of torque. Due to this, size and weight reduction of the component parts has been achieved.