SAS CONTROL MODULE CONFIGURATION

id081000801500

  Note
  • Use the IDS (laptop PC) because the PDS (Pocket PC) does not support the SAS CONTROL MODULE CONFIGURATION.

1. Connect the M-MDS to the DLC-2.

2. After the vehicle is identified, select the following items from the initialization screen of the M-MDS.

  • When using the IDS (laptop PC)
    1. Select “Module Programming”.

3. Then, select items from the screen menu in the following order.

  1. Select “Programmable Module Installation”.
  2. Select “RCM”.

4. Perform the configuration according to the directions on the screen.

5. Retrieve DTCs by the M-MDS, then verify that there is no DTC present.

  • If a DTC (s) is detected, perform the applicable DTC inspection. (See DTC TABLE.)