REAR DOOR CHECKER REMOVAL/INSTALLATION

id091100520700

1. Fully close the rear door glass.

2. Disconnect the negative battery cable.

3. Remove the following parts:

  (1) Inner sail garnish (See INNER SAIL GARNISH REMOVAL/INSTALLATION.)

  (2) Rear door trim (See REAR DOOR TRIM REMOVAL/INSTALLATION.)

  (3) Rear door speaker (See REAR DOOR SPEAKER REMOVAL/INSTALLATION.)

4. Remove in the order indicated in the table.

ac9wzw00002484

1 | Bolt A
2 | Bolt B
3 | Rear door checker
4 | Rear door

5. Install in the reverse order of removal.

6. Adjust the front door. (See DOOR ADJUSTMENT.)