REAR HEAT DUCT COMPONENT REMOVAL/INSTALLATION

id071100802800

Rear Heat Duct No.1

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Front seat (See FRONT SEAT REMOVAL/INSTALLATION.)

  (2) Front scuff plate inner (See FRONT SCUFF PLATE REMOVAL/INSTALLATION.)

  (3) Front side trim (See FRONT SIDE TRIM REMOVAL/INSTALLATION.)

  (4) Decoration panel (See DECORATION PANEL REMOVAL/INSTALLATION.)

  (5) Front console box mat (See FRONT CONSOLE BOX MAT REMOVAL/INSTALLATION.)

  (6) Indicator panel (See INDICATOR PANEL REMOVAL/INSTALLATION.)

  (7) Front console box (See FRONT CONSOLE BOX REMOVAL/INSTALLATION.)

  (8) Dashboard under cover (See DASHBOARD UNDER COVER REMOVAL/INSTALLATION.)

  (9) Side wall (See SIDE WALL REMOVAL/INSTALLATION.)

  (10) Console panel (See CONSOLE PANEL REMOVAL/INSTALLATION.)

  (11) Console cover (See CONSOLE COVER REMOVAL/INSTALLATION.)

  (12) Console (See CONSOLE REMOVAL/INSTALLATION.)

  (13) Dust cover (See STEERING WHEEL AND COLUMN REMOVAL/INSTALLATION.)

3. Turn floor covering over. (See FLOOR COVERING REMOVAL/INSTALLATION.)

4. Remove in the order indicated in the table.

ac9uuw00000781

1 | Fastener
2 | Rear heat duct No.1 (RH)
3 | Rear heat duct No.1 (LH)

5. Install in the reverse order of removal.

Rear heat duct No.2, No.3 and No.4

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Decoration panel (See DECORATION PANEL REMOVAL/INSTALLATION.)

  (2) Front console box mat (See FRONT CONSOLE BOX MAT REMOVAL/INSTALLATION.)

  (3) Indicator panel (See INDICATOR PANEL REMOVAL/INSTALLATION.)

  (4) Front console box (See FRONT CONSOLE BOX REMOVAL/INSTALLATION.)

  (5) Dashboard under cover (See DASHBOARD UNDER COVER REMOVAL/INSTALLATION.)

  (6) Side wall (See SIDE WALL REMOVAL/INSTALLATION.)

  (7) Console panel (See CONSOLE PANEL REMOVAL/INSTALLATION.)

  (8) Console cover (See CONSOLE COVER REMOVAL/INSTALLATION.)

  (9) Console (See CONSOLE REMOVAL/INSTALLATION.)

  (10) Second-row seat (See SECOND-ROW SEAT REMOVAL/INSTALLATION.)

  (11) Edge cover (See LONG SLIDER REMOVAL/INSTALLATION.)

  (12) Long slider cover (See LONG SLIDER REMOVAL/INSTALLATION.)

  (13) Third-row seat (See THIRD-ROW SEAT REMOVAL/INSTALLATION.)

  (14) Trunk box (See TRUNK BOX REMOVAL/INSTALLATION.)

  (15) Seat side box (See SEAT SIDE BOX REMOVAL/INSTALLATION.)

  (16) Trunk end trim (See TRUNK END TRIM REMOVAL/INSTALLATION.)

  (17) Third-row seat (See THIRD-ROW SEAT REMOVAL/INSTALLATION.)

  (18) Rear scuff plate inner (See REAR SCUFF PLATE REMOVAL/INSTALLATION.)

  (19) Third-row seat belt lower anchor installation bolt (See THIRD-ROW SEAT BELT REMOVAL/INSTALLATION.)

  (20) Trunk side trim (See TRUNK SIDE TRIM REMOVAL/INSTALLATION.)

3. Remove the two rear A/C unit retaining bolts on the rear side.

4. Turn floor covering over. (See FLOOR COVERING REMOVAL/INSTALLATION.)

5. Remove the long slider. (See LONG SLIDER REMOVAL/INSTALLATION.)

6. Remove the fasteners.

ac9wzw00002792

7. Lift the rear side of the rear A/C unit and remove the rear heater duct No.2.

8. Remove the rear heat duct No.3.

9. Remove the rear heat duct No.4.

10. Install in the reverse order of removal.

When removing the rear heater duct No.3 only

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Second-row seat (LH) (See SECOND-ROW SEAT REMOVAL/INSTALLATION.)

  (2) Edge cover (See LONG SLIDER REMOVAL/INSTALLATION.)

  (3) Long slider cover (See LONG SLIDER REMOVAL/INSTALLATION.)

3. Cut away the floor covering as shown in the figure.

ac9wzw00002793

  Note
  • The cut part does not need to match up when installing the floor covering.

4. Turn floor covering over.

ac9uuw00000783

5. Remove the rear heat duct No.3.

6. Install in the reverse order of removal.

When removing the rear heater duct No.4 only

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Second-row seat (RH) (See SECOND-ROW SEAT REMOVAL/INSTALLATION.)

  (2) Edge cover (See LONG SLIDER REMOVAL/INSTALLATION.)

  (3) Long slider cover (See LONG SLIDER REMOVAL/INSTALLATION.)

3. Cut away the floor covering as shown in the figure.

ac9uuw00000953

  Note
  • The cut part does not need to match up when installing the floor covering.

4. Turn floor covering over.

ac9uuw00000954

5. Remove the rear heat duct No.4.

6. Install in the reverse order of removal.