ACTIVE COMMAND MODES TABLE [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 10-PIN TYPE]

id0902q3960900

BSM Control Module (LH)

Simulation item | Unit/Operation | Data contents | Output part name
--- | --- | --- | ---
BSM_OFF_IL | On/Off | • On: Illuminates BSM OFF indicator light. • Off: Turns off BSM OFF indicator light. | BSM OFF indicator light (Instrument cluster)
Buzzer | On/Off | • On: Operates BSM warning alarm. • Off: Stops BSM warning alarm. | BSM warning alarm (Instrument cluster)
IL_MODE | Off/On | • Off: Illuminates BSM OFF indicator light in night mode. • On: Illuminates BSM OFF indicator light in daytime mode. | BSM OFF indicator light (Instrument cluster)
RCTA_BUZZER | Off/On | • Off: RCTA warning alarm does not sound. • On: RCTA warning alarm sounds. | RCTA warning alarm (Instrument cluster)
RCTA_WARN | Off/On | • Off: Turn off RCTA indicator lights. • On: Illuminate RCTA indicator lights. Note • BSM indicator lights will be turned on, if the selector lever is in R position. | • RCTA indicator light (Audio unit) • BSM indicator light (Power outer mirror)
VSPD | OFF/ON | • OFF: Does not input vehicle speed. • ON: Inputs vehicle speed of 34 km/h {21 mph}. | BSM control module (LH)
WRN_IND_L | Off/On | • Off: Turns off BSM indicator light (LH). • On: Illuminates BSM indicator light (LH). | BSM indicator light (LH) (Power outer mirror (LH))

BSM Control Module (RH)

Simulation item | Unit/Operation | Data contents | Output part name
--- | --- | --- | ---
IL_MODE | Off/On | • Off: Illuminates BSM OFF indicator light in night mode. • On: Illuminates BSM OFF indicator light in daytime mode. | BSM OFF indicator light (Instrument cluster)
RCTA_BUZZER | Off/On | • Off: RCTA warning alarm does not sound. • On: RCTA warning alarm sounds. | RCTA warning alarm (Instrument cluster)
RCTA_WARN | Off/On | • Off: Turn off RCTA indicator lights. • On: Illuminate RCTA indicator lights. Note • BSM indicator lights will be turned on, if the selector lever is in R position. | • RCTA indicator light (Audio unit) • BSM indicator light (Power outer mirror)
VSPD | OFF/ON | • OFF: Does not input vehicle speed. • ON: Inputs vehicle speed of 34 km/h {21 mph}. | BSM control module (RH)
WRN_IND_R | Off/On | • Off: Turns off BSM indicator light (RH). • On: Illuminates BSM indicator light (RH). | BSM indicator light (RH) (Power outer mirror (RH))