THEFT-DETERRENT SYSTEM OUTLINE [WITH INTRUDER SENSOR]

id0914001005b7

• The theft-deterrent system operates the siren and the hazard warning lights if a door, liftgate or the bonnet is improperly opened, or if its sensor detects movement from an intrusion into the vehicle such as a window being broken.
• Signal input/output of the theft-deterrent system is controlled by the theft-deterrent system control module.