FUEL PUMP UNIT INSPECTION [MZI-3.7]

id0114d2801100

Continuity Inspection

1. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [MZI-3.7].)

2. To remove the service hole cover, remove the following parts:

  (1) Second-row seat (See SECOND-ROW SEAT REMOVAL/INSTALLATION.)

  (2) Edge cover (See LONG SLIDER REMOVAL/INSTALLATION.)

  (3) Long slider cover (See LONG SLIDER REMOVAL/INSTALLATION.)

  (4) Rear heat duct No.3 (See REAR HEAT DUCT COMPONENT REMOVAL/INSTALLATION.)

  (5) Service hole cover (See FUEL PUMP UNIT REMOVAL/INSTALLATION [MZI-3.7].)

3. Disconnect the fuel pump unit connector.

4. Inspect for continuity between fuel pump unit connector terminals B and D.

ac9wzw00002155

  • If there is no continuity, replace the fuel pump unit. (See FUEL PUMP UNIT REMOVAL/INSTALLATION [MZI-3.7].)