DTC C1280, C1282, C1516, C2770

id080200820700

DTC | C1280 | Yaw rate sensor in SAS control module is signal error
--- | --- | ---
C1282 | Low-G (XY) sensor (lateral-G) in SAS control module is signal error
C1516 | Roll rate sensor in SAS control module is signal error
C2770 | Low-G (XY) sensor (forward-G) in SAS control module is signal error
DETECTION CONDITION | Warning • Detection conditions are for understanding the DTC outline before performing an inspection. Performing an inspection with only detection conditions may cause injury due to an operating error, or damage the system. When performing an inspection, always follow the inspection procedure. • Malfunction in the SAS control module
POSSIBLE CAUSE | • SAS control module malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | PERFORM SAS CONTROL MODULE DTC INSPECTION • Clear the DTC for the SAS control module using the M-MDS. (See CLEARING DTC.) • Perform the DTC inspection for the SAS control module using the M-MDS. (See DTC DISPLAY.) • Are the same DTCs present? | Yes | Replace the SAS control module. (See SAS CONTROL MODULE REMOVAL/INSTALLATION.)
No | DTC troubleshooting completed.