TWEETER REMOVAL/INSTALLATION

id092000808000

1. Disconnect the negative battery cable.

2. Remove the cover from the dashboard using a flathead screwdriver wrapped with protective tape.

3. Remove the solar radiation sensor. (See SOLAR RADIATION SENSOR REMOVAL/INSTALLATION.) (LH only)

4. Remove in the order indicated in the table.

ac9uuw00001395

1 | Screw
2 | Tweeter
3 | Connector

5. Install in the reverse order of removal.