FRONT AIR MIX ACTUATOR REMOVAL/INSTALLATION

id074000805800

Driver Side

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Dashboard under cover (Driver side) (See DASHBOARD UNDER COVER REMOVAL/INSTALLATION.)

  (2) Side wall (See SIDE WALL REMOVAL/INSTALLATION.)

  (3) Console panel (LH) (See CONSOLE PANEL REMOVAL/INSTALLATION.)

  (4) Bonnet release lever (See BONNET LATCH AND RELEASE LEVER REMOVAL/INSTALLATION.)

  (5) Lower panel (See LOWER PANEL REMOVAL/INSTALLATION.)

3. Remove in the order indicated in the table.

L.H.D.

ac9wzw00002816

R.H.D.

ac9wzw00002817

1 | Driver-side front air mix actuator connector
2 | Screw
3 | Driver-side front air mix actuator

4. Install in the reverse order of removal.

Passenger Side

L.H.D.

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Decoration panel (See DECORATION PANEL REMOVAL/INSTALLATION.)

  (2) Front console box mat (See FRONT CONSOLE BOX MAT REMOVAL/INSTALLATION.)

  (3) Indicator panel (See INDICATOR PANEL REMOVAL/INSTALLATION.)

  (4) Front console box (See FRONT CONSOLE BOX REMOVAL/INSTALLATION.)

  (5) Dashboard under cover (See DASHBOARD UNDER COVER REMOVAL/INSTALLATION.)

  (6) Side wall (See SIDE WALL REMOVAL/INSTALLATION.)

  (7) Console panel (See CONSOLE PANEL REMOVAL/INSTALLATION.)

  (8) Console cover (See CONSOLE COVER REMOVAL/INSTALLATION.)

  (9) Console (See CONSOLE REMOVAL/INSTALLATION.)

  (10) Front scuff plate inner (See FRONT SCUFF PLATE REMOVAL/INSTALLATION.)

  (11) Front side trim (See FRONT SIDE TRIM REMOVAL/INSTALLATION.)

  (12) Glove compartment (See GLOVE COMPARTMENT REMOVAL/INSTALLATION.)

  (13) Bonnet release lever (See BONNET LATCH AND RELEASE LEVER REMOVAL/INSTALLATION.)

  (14) Lower panel (See LOWER PANEL REMOVAL/INSTALLATION.)

  (15) Lower column cover (See COLUMN COVER REMOVAL/INSTALLATION.)

  (16) Driver-side air bag module (See DRIVER-SIDE AIR BAG MODULE REMOVAL/INSTALLATION.)

  (17) Steering wheel (See STEERING WHEEL AND COLUMN REMOVAL/INSTALLATION.)

  (18) Combination switch (See COMBINATION SWITCH REMOVAL/INSTALLATION.)

  (19) Center panel (See CENTER PANEL REMOVAL/INSTALLATION.)

  (20) Meter hood (See METER HOOD REMOVAL/INSTALLATION.)

  (21) Instrument cluster (See INSTRUMENT CLUSTER REMOVAL/INSTALLATION.)

  (22) Audio unit (See AUDIO UNIT REMOVAL/INSTALLATION.)

  (23) Steering shaft (See STEERING WHEEL AND COLUMN REMOVAL/INSTALLATION.)

  (24) A-pillar trim (See A-PILLAR TRIM REMOVAL/INSTALLATION.)

  (25) Side panel (See SIDE PANEL REMOVAL/INSTALLATION.)

  (26) Passenger-side air bag module (R.H.D.) (See PASSENGER-SIDE AIR BAG MODULE REMOVAL/INSTALLATION.)

3. Disconnect the front door wiring harness connector (Driver side). (See FRONT DOOR MODULE PANEL REMOVAL/INSTALLATION.)

4. Disconnect the dashboard harness connectors.

5. Remove the brake switch from the brake pedal with the brake switch connector connected. (See BRAKE PEDAL REMOVAL/INSTALLATION [L.H.D.].) (See BRAKE PEDAL REMOVAL/INSTALLATION [R.H.D.].)

6. Remove the selector lever component. (See SELECTOR LEVER COMPONENT REMOVAL/INSTALLATION.)

7. Remove the windshield wiper arm and blade. (See WINDSHIELD WIPER ARM AND BLADE REMOVAL/INSTALLATION.)

8. Remove the cowl grille. (See COWL GRILLE REMOVAL/INSTALLATION.)

9. Remove the windshield wiper motor. (See WINDSHIELD WIPER MOTOR REMOVAL/INSTALLATION.)

10. Remove the dashboard. (See DASHBOARD REMOVAL/INSTALLATION.)

11. Remove in the order indicated in the table.

ac9uuw00001040

1 | Passenger-side front air mix actuator connector
2 | Screw
3 | Passenger-side front air mix actuator

12. Install in the reverse order of removal.

R.H.D.

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Dashboard under cover (passenger side) (See DASHBOARD UNDER COVER REMOVAL/INSTALLATION.)

  (2) Glove compartment service hole cover (See AIR FILTER REMOVAL/INSTALLATION.)

  (3) Glove compartment (See GLOVE COMPARTMENT REMOVAL/INSTALLATION.)

  (4) Fuse block

3. Remove in the order indicated in the table.

ac9wzw00002818

1 | Passenger-side front air mix actuator connector
2 | Screw (See Screw installation note.)
3 | Passenger-side front air mix actuator

4. Install in the reverse order of removal.

Screw installation note

1. Install the screw on the end of the Phillips screwdriver with the packing tape.

ac9wzw00001708

2. Install the screw to the front air mix actuator.

3. Pull out the Phillips screwdriver together with the packing tape.