SECURITY AND LOCKS PERSONALIZATION FEATURES

id091400590200

• A personalization features that switches the activation/deactivation of each function has been adopted.
• The setting of the following system functions, and warning and guidance functions can be turned ON/OFF optionally.
• Refer to the Workshop Manual for the detailed setting procedure.

Using Mazda Modular Diagnostic System (M-MDS)

Mazda Modular Diagnostic System (M-MDS) display | Function | Initial setting | Setting content | Control unit
--- | --- | --- | --- | ---
Answer Back Buzzer | Answer back buzzer function can be set. | Enabled | Disabled/ Enabled | Keyless control module
Card key battery low warning | Advanced key remaining battery level/battery dead warning can be set. | Enabled | Disabled/ Enabled | Keyless control module
Automatic Locks | Automatic locks function can be set. | Disabled | Disabled/ Enabled | Keyless control module
Two(2) stage door unlocking by request switch. | 2-step unlocking system can be set. | Enabled | Disabled/ Enabled | Keyless control module
Two(2) stage door unlocking by transmitter. | 2-step unlocking system can be set. | Enabled | Disabled/ Enabled | Keyless control module
Auto relock timer (with AKE) | The operation start time of the auto re-lock function can be changed. | 60s | 30s/60s/90s | Keyless control module

Setting Method By Operation Of Door Lock Switch (With Auto Door Lock System)

Setting content | Function | Initial setting | Control unit
--- | --- | --- | ---
Disabled | Auto lock/unlock function can be changed. | Auto door lock operation based on vehicle speed. Auto door unlock operation based on ignition switch position. | BCM
Auto door lock operation based on vehicle speed.
Auto door lock operation based on vehicle speed. Auto door unlock operation based on ignition switch position.
Auto door lock operation based on shift position.
Auto door lock operation based on shift position. Auto door unlock operation based on shift position.