AIR INTAKE ACTUATOR REMOVAL/INSTALLATION

id074000801400

1. Disconnect the negative battery cable.

2. Remove the dashboard under cover. (Passenger side) (See DASHBOARD UNDER COVER REMOVAL/INSTALLATION.)

3. Remove the glove compartment. (See GLOVE COMPARTMENT REMOVAL/INSTALLATION.)

4. Insert a flathead screwdriver as shown in the figure and detach the fuse block tab by prying it in the direction of the arrow.

ac9uuw00001119

5. Press the fuse block and remove it from the bracket.

6. Set the fuse block out of the way.

7. Remove in the order indicated in the table.

L.H.D.

ac9wzw00002798

R.H.D.

ac9wzw00002799

1 | Air intake actuator connector
2 | Screw
3 | Air intake actuator

8. Install in the reverse order of removal.