REFRIGERANT PRESSURE SENSOR REMOVAL/INSTALLATION

id074000817300

1. Disconnect the negative battery cable.

2. Discharge the refrigerant. (See REFRIGERANT CHARGING.)

3. Disconnect the refrigerant pressure sensor connector.

  Caution
  • If moisture or foreign material enters the refrigeration cycle, cooling ability will be lowered and abnormal noise will occur. Always immediately plug all open fittings after removing any refrigeration cycle parts to keep moisture or foreign material out of the cycle.

4. Loosen the refrigerant pressure sensor using two spanners.

5. Remove the refrigerant pressure sensor. (See Refrigerant Pressure Sensor Installation Note.)

ac9wzw00002821

  Tightening torque

  10—11 N·m {102—112 kgf·cm, 89—97 in·lbf}

6. Install in the reverse order of removal.

7. Perform the refrigerant system performance test. (See REFRIGERANT SYSTEM PERFORMANCE TEST.)

Refrigerant Pressure Sensor Installation Note

1. Apply compressor oil to the O-rings and connect the joints.