CONSOLE REMOVAL/INSTALLATION

id091700801200

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Decoration panel (See DECORATION PANEL REMOVAL/INSTALLATION.)

  (2) Front console box mat (See FRONT CONSOLE BOX MAT REMOVAL/INSTALLATION.)

  (3) Indicator panel (See INDICATOR PANEL REMOVAL/INSTALLATION.)

  (4) Front console box (See FRONT CONSOLE BOX REMOVAL/INSTALLATION.)

  (5) Dashboard under cover (See DASHBOARD UNDER COVER REMOVAL/INSTALLATION.)

  (6) Side wall (See SIDE WALL REMOVAL/INSTALLATION.)

  (7) Console panel (See CONSOLE PANEL REMOVAL/INSTALLATION.)

  (8) Console cover (See CONSOLE COVER REMOVAL/INSTALLATION.)

3. Remove the screws.

ac9wzw00001240

4. Remove the bolts.

5. Disconnect the accessory socket connector and auxiliary jack connector, and keyless antenna connector.

6. Remove the console in the direction of the arrow.

7. Install in the reverse order of removal.