DTC B2937 [POWER LIFTGATE (PLG) SYSTEM]

id0902e9381100

DTC B2937 | PLG motor circuit malfunction
--- | ---
DETECTION CONDITION | PLG motor current is excessively low. (less than 1A)
POSSIBLE CAUSE | • Open circuit in wiring harness between PLG control module terminal 1E and PLG motor terminal A (PLG drive unit) • Open circuit in wiring harness between PLG control module terminal 1F and PLG motor terminal B (PLG drive unit) • PLG motor malfunction • PLG control module malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | INSPECT WIRING HARNESS BETWEEN PLG CONTROL MODULE AND PLG DRIVE UNIT • Disconnect the PLG control module connector. • Disconnect the PLG drive unit connector. • Inspect the wiring harness between PLG control module terminals 1E and 1F, and PLG drive unit terminals A and B for an open circuit. • Is the wiring harness normal? | Yes | Replace the PLG drive unit. (See POWER LIFTGATE (PLG) DRIVE UNIT REMOVAL/INSTALLATION.) Go to the next step.
No | Repair or replace the wiring harness. Go to the next step.
2 | VERIFY CORRECTION COMPLETED • Reconnect the disconnected connector. • Clear the DTC. • Operate the PLG system. • Is DTC B2937 stored? | Yes | Replace the PLG control module. (See POWER LIFTGATE (PLG) CONTROL MODULE REMOVAL/INSTALLATION.)
No | DTC troubleshooting completed.