- SYMPTOM TROUBLESHOOTING CHART [POWER WINDOW SYSTEMS (EXTERIOR OPEN/CLOSE FUNCTION)]
- QUICK DIAGNOSTIC CHART [POWER WINDOW SYSTEMS (EXTERIOR OPEN/CLOSE FUNCTION)]
- No.1 DOOR GLASS DOES NOT OPERATE EVEN THOUGH VARIOUS OPERATIONS ARE PERFORMED [POWER WINDOW SYSTEMS (EXTERIOR OPEN/CLOSE FUNCTION)]
- No.2 DOOR GLASS DOES NOT OPERATE USING THE KEYLESS TRANSMITTER [POWER WINDOW SYSTEMS (EXTERIOR OPEN/CLOSE FUNCTION)]
- No.3 DOOR GLASS DOES NOT OPERATE USING THE REQUEST SWITCH [POWER WINDOW SYSTEMS (EXTERIOR OPEN/CLOSE FUNCTION)]
- No.4 SOME DOOR GLASS DO NOT OPERATE [POWER WINDOW SYSTEMS (EXTERIOR OPEN/CLOSE FUNCTION)]
- No.5 DOOR GLASS STOPS BEFORE FULLY OPENING/CLOSING [POWER WINDOW SYSTEMS (EXTERIOR OPEN/CLOSE FUNCTION)]
- No.6 DOOR GLASS REVERSES BEFORE IT FULLY CLOSES [POWER WINDOW SYSTEMS (EXTERIOR OPEN/CLOSE FUNCTION)]
- No.7 ALL DOOR GLASS OPERATE ACCIDENTALLY [POWER WINDOW SYSTEMS (EXTERIOR OPEN/CLOSE FUNCTION)]
- No.8 PART OF DOOR GLASS OPERATES ACCIDENTALLY [POWER WINDOW SYSTEMS (EXTERIOR OPEN/CLOSE FUNCTION)]