HEADLIGHT CLEANER HOSE REMOVAL/INSTALLATION

id091900803100

1. Disconnect the negative battery cable.

2. Remove the front bumper. (See FRONT BUMPER REMOVAL/INSTALLATION.)

3. Disconnect the headlight cleaner hose from the joint pipe.

ac9wzw00002842

4. Disconnect the headlight cleaner hose from the headlight cleaner actuator.

5. Remove the bracket from the front bumper rib.

6. Remove the clips from the front bumper.

7. Install in the reverse order of removal.