TRUNK SIDE TRIM REMOVAL/INSTALLATION

id091700803100

Driver Side

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Trunk box (See TRUNK BOX REMOVAL/INSTALLATION.)

  (2) Seat side box (See SEAT SIDE BOX REMOVAL/INSTALLATION.)

  (3) Trunk end trim (See TRUNK END TRIM REMOVAL/INSTALLATION.)

  (4) Third-row seat (See THIRD-ROW SEAT REMOVAL/INSTALLATION.)

  (5) Rear scuff plate inner (Driver Side) (See REAR SCUFF PLATE REMOVAL/INSTALLATION.)

  (6) Third-row seat belt lower anchor installation bolt (Driver Side) (See THIRD-ROW SEAT BELT REMOVAL/INSTALLATION.)

3. Pull the cup holder upward and detach clips A, pins B, and tabs C.

4. Remove the cup holder.

5. Remove the bolts, and remove the cargo net hook.

6. Remove the cover.

7. Remove the screw.

8. Remove the bolt.

9. Pull the trunk side trim outward and detach clips D, tabs E, and pin F.

10. Remove the trunk side trim.

11. Install in the reverse order of removal.

ac9wzw00000638

Passenger Side

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Trunk box (See TRUNK BOX REMOVAL/INSTALLATION.)

  (2) Seat side box (See SEAT SIDE BOX REMOVAL/INSTALLATION.)

  (3) Trunk end trim (See TRUNK END TRIM REMOVAL/INSTALLATION.)

  (4) Third-row seat (See THIRD-ROW SEAT REMOVAL/INSTALLATION.)

  (5) Rear scuff plate inner (Passenger Side) (See REAR SCUFF PLATE REMOVAL/INSTALLATION.)

  (6) Third-row seat belt lower anchor installation bolt (Passenger Side) (See THIRD-ROW SEAT BELT REMOVAL/INSTALLATION.)

3. Pull the cup holder upward and detach clips A, pins B, and tabs C.

4. Remove the cup holder.

5. Remove the bolts, and remove the cargo net hook.

6. Remove the cover.

7. Remove the screw.

8. Remove the bolt.

9. Pull the trunk side trim outward and detach clips D, tabs E, and pin F.

10. Disconnect the accessory socket connector.

11. Remove the trunk side trim.

12. Install in the reverse order of removal.

ac9wzw00000639