ADVANCED KEYLESS ENTRY SYSTEM FUNCTION

id091400595200

• If the system is operated improperly, it warns the driver using the indicator light in the instrument cluster, beeper sound, and keyless beeper in the front fender.
• The operation condition of the advanced keyless system is indicated by the indicator light and beeper sound to guide user’s operation.

Item | Operation condition | Keyless beeper (outside the vehicle) | Instrument cluster
--- | --- | --- | ---
Buzzer (Interior) | Keyless warning light (red) | Keyless indicator light (green)
Warning | Start knob not in LOCK warning | Driver’s door is open with start knob in ACC position | − | Continuous | Flashes | −
Advanced key out of vehicle warning*1 | Advanced key cannot be detected inside vehicle with driver’s door open and start knob not in OFF position | − | Continuous | Flashes*2 | −
Advanced key cannot be detected inside vehicle with all doors closed and start knob not in OFF position | Sounds 6 times | ― | Flashes*3 | −
Advanced key cannot be detected inside vehicle with start knob not in OFF position and under any condition other than above | − | ― | Flashes*2 | −
Advanced key left in vehicle warning | Door/trunk lid is open with proper advanced key inside vehicle and another advanced key carried | Continuous for 10 s | − | − | −
Door lock inoperable warning | Request switch is pressed with advanced key carried and a door open or start knob not in OFF position | Sounds 6 times | − | − | −
Battery voltage low indication | Advanced key battery voltage depleted | − | − | − | Flashes (Approx. 30 s after IG OFF)
Guidance | Start knob operable guidance | Start knob is operable (lock released) when it is pressed | − | − | − | On (Max. 3 s)
Start knob inoperable guidance | Start knob is inoperable (locked) when it is pressed | − | − | Flashes | −
Lock/unlock answer back | Doors are locked/unlocked with normal/advanced keyless entry function | Locked: Once Unlocked: Twice | − | − | −

*1 :If the start knob is turned to the OFF position with the advanced key out of the vehicle, the start knob is inoperable (the engine cannot be restarted). For vehicles with the immobilizer system, the engine cannot be restarted by turning the start knob from the ACC position to the START position even though the start knob has not been turned to the OFF position.
*2 :Stops flashing and goes out if the advanced key is detected inside the vehicle.
*3 :Stops flashing and goes out if the advanced key is detected inside the vehicle and door is opened.